|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Address | | **INSPECTIONS OF LADDERS**  **Ref:**  **Ladder Identification Number:** | | | | Logo |
| **VISUAL CHECKS** | **WOOD** | | **METAL** | **FIBREGLASS** | **PASSED** | **FAILED**  **(Notes)** |
| Rungs for splintering |  | |  |  |  |  |
| Rungs for tightness |  | |  |  |  |  |
| Rungs for cracks |  | |  |  |  |  |
| Evidence of rot |  | |  |  |  |  |
| Tie rods |  | |  |  |  |  |
| Retaining hooks |  | |  |  |  |  |
| Check guides |  | |  |  |  |  |
| Check head for soundness |  | |  |  |  |  |
| Check feet for damage |  | |  |  |  |  |
| Check strings |  | |  |  |  |  |
| Check sides for bowing |  | |  |  |  |  |
| Check for cracks |  | |  |  |  |  |
| Check for splinters |  | |  |  |  |  |
| Any other visual damage |  | |  |  |  |  |
| Ladders locked |  | |  |  |  |  |
| Pulley systems working |  | |  |  |  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| General checks at working angle: |  |  |  |  |  |
| Note: during checks, ladders head and feet must be carefully secured. |  |  |  |  |  |
| Unique identification visible. |  |  |  |  |  |