|  |
| --- |
| **OXY-ACETYLENE WELDING EQUIPMENT** |
| **Unit No:** | **Type:** | **Shift:** | **Operator:** |
| **Item** |  | **(√)** |
| **Mounting** **Fittings** | Bottles are upright and secure |  |
| Secure with no leaks |  |
| **Blowpipe, Cutting / Welding Attachments** | No cracking |  |
| Good condition of seals, seats. |  |
| **Flashback arrestors** | Fitted to torch and regulators |  |
| General condition good |  |
| **Hoses and Fittings** | No burns, cracking or deterioration |  |
| General condition good |  |
| **Regulators** | O-ring condition good |  |
| Gauges operating / condition |  |
| **Oil and Grease** | All equipment free of oil and grease contamination |  |
| **Emergency equipment** | Fire extinguisher readily available |  |
| **Regulator valves within date**  | Valves should be date stamped and with in a 4year life cycle  |  |
| **Comments:** |
| **Inspected by Team member (Competent person)** | **Approved by Team Leader** |
| **Print Name**: ………………………………………….**Signed:** …………………………….……………..….**Date:**……………………………..…………………… | **Print Name**: …………….……..…………………..**Signed:** ……………………..……………………..**Date:** ………………………………………………… |